**The Farmax ERP is a spader for light tractors. The great manoeuvrability and low integral weight of the ERP make it highly suitable for use in greenhouse horticulture, fl ower cultivation and tilling small plots.**

Apart from giving perfect rotavation, the popularity of the Farmax ERP is mainly attributable to its ease of operation and sturdy design.



**www.farmax.info**

Wasse BV | Oranjekanaal Zuidzijde 17 | 9415 PR Hijken | Netherlands | Tel: +31 (0)593 524 066 | www.wasse.nl | info@wasse.nl

# Uninterrupted rotavation

The ERP is fi tted as standard with skimmers to prevent the tilled soil from clogging the machine. The machine can be combined with a rotary harrow.

|  |
| --- |
| ERP spader |

**Drive:** Single-sided chain transmission

**Tractor power:** 20 to 35 HP **Power take-off revs:** 540 r.p.m.

# Advantages

* low power requirement, so suitable for small tractors

**www.farmax.info**

Wasse BV | Oranjekanaal Zuidzijde 17 | 9415 PR Hijken | Netherlands | Tel: +31 (0)593 524 066 | www.wasse.nl | info@wasse.nl

* highly manoeuvrable, even in small spaces
* easy to operate
* sturdy, low-maintenance design
* improved yield thanks to improved soil structure

*Also available without rotary harrow*

*Rotary harrow ensures an*

*optimum bed for sowing*




*With light transmission case*



*Mechanical adjustment of*

*the rotary harrow*



# Technical Data

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **type** | **operating width** | **max.**  **operating depth** | **standard**  **weight** | **required power kW/HP** | **number**  **of spades** |
| ERP 90 | 35.43” - 90 cm | 17.72” - 45 cm | 573 Lbs - 260 kg | 13/18 | 12 |
| ERP 105 | 41.34” - 105 cm | 17.72” - 45 cm | 650 Lbs - 295 kg | 15/20 | 12 |
| ERP 125 | 49.21” - 125 cm | 17.72” - 45 cm | 760 Lbs - 345 kg | 16/21 | 12 |
| ERP 140 | 55.12” - 140 cm | 17.72” - 45 cm | 870 Lbs - 395 kg | 21/28 | 12 |
| ERP 155 | 61.02” - 155 cm | 17.72” - 45 cm | 992 Lbs - 450 kg | 22/30 | 12 |